**Akai LPD8 – Remix Deck Mapping**

*This mapping requires Traktor Pro 2.6.2 or higher*

Since the LPD8 is limited to the number of pads and programs, it only has the ability to control Cells 1-8. This still allows you to control up to 32 samples per Remix Deck. This mapping uses the default presets that came with the LPD8. If you have modified the presets you will need to download the LPD8 Editor and load the preset included.

**Editor Setup**

In order for this mapping work correctly within Traktor you will first need to load the default MIDI settings to the LPD8 using the LPD8 Editing Software.

1. Download the Editing Software from <http://www.akaipro.com/lpd8>
2. Install and Open the Editor.
3. Select the LPD8 from the drop down list.
4. Click Load Preset from the top.
5. Select the Akai LPD8 - Traktor Remix Decks Preset file.
6. Click Ok to Load Settings.
7. Click Commit - Upload to send the settings to the LPD8.
8. Open Traktor and Import the LPD8 Remix Deck [C/D] v1.0 tsi File.

**Traktor Setup**

1. Open Traktor Pro 2.6.2 Software.
2. Click the **Preferences** or **gear** icon from the top right menu.
3. Select **Controller Manager** from the list on the left.
4. Click the **Add… > Import** from **Device Setup**.   
     
   
5. Browse your computer to locate the **LPD8 Remix Deck.tsi** mapping file.  
     
   
6. Ensure that the **LPD8** is selected as your **In-Port**, and **Out-Port**.
7. To change cells press **Program**, and then press one of the 4 lower pads.
8. Once you have selected the Program or Cell section press **Pad** to exit Program mode.   
     
   